**Bike Assembly Steps**

* Take bike out of box
* Remove packaging from bike
* Clamp bike in stand
* Hang front tire loosely in forks
* Insert stem and handlebars loosely into fork tube
* Tighten seat to seat post
* Insert seat and seat post into downtube
* Insert and tighten pedals into crank arms using pedal wrench
* Tighten front wheel centered in forks using impact wrench
* Tighten handlebar clamp with handlebars properly centered using impact wrench
* Tighten stem bolt and wedge nut with handlebars properly aligned using impact wrench
* Tighten seat and seat post with seat properly aligned using impact wrench
* Adjust and tighten all brake levers and shifters using drill
* Install and tighten reflectors using drill
* Adjust front brakes
* True front wheel
* Adjust front derailleur
* Adjust rear derailleur
* Adjust rear brakes
* True rear wheel
* Air up tires
* Attach any and all accessories
* Place ID sticker on back side of downtube above crank
* Remove bike from stand
* Perform safety check of parts attached
* Squeeze brake levers to make sure they are working properly
* Put front tire between knees and make sure handlebars are tight
* Visually check pedals are tighten fully
* Stage bike for store